Table of Contents

[Table of Contents 1](#_Toc184699)

[1 TdmContainer 2](#_Toc184700)

[1.1 TdmContainerCurrentProblems 2](#_Toc184701)

[1.2 MW\_TdmContainer\_Pac 2](#_Toc184702)

[1.3 TdmContainerCapability 4](#_Toc184703)

[1.4 TdmContainerConfiguration 5](#_Toc184704)

[1.5 TdmContainerHistoricalPerformances 6](#_Toc184705)

[1.6 TdmContainerStatus 7](#_Toc184706)

[1.7 TdmContainerCurrentPerformance 8](#_Toc184707)

[2 Data Types 9](#_Toc184708)

[2.1 ContainerCurrentPerformanceType 9](#_Toc184709)

[2.2 ContainerCurrentProblemType 9](#_Toc184710)

[2.3 ContainerHistoricalPerformanceType 9](#_Toc184711)

[2.4 ContainerPerformanceType 10](#_Toc184712)

[2.5 ContainerProblemSeverityType 11](#_Toc184713)

[2.6 ContainerType 12](#_Toc184714)

[2.7 SegmentIDType 13](#_Toc184715)

[2.8 SegmentStatusType 13](#_Toc184716)

[2.9 TdmContainerType 14](#_Toc184717)

[2.10 TdmStructureType 15](#_Toc184718)

[3 Enumeration Types 16](#_Toc184719)

[3.1 GranularityPeriodType 16](#_Toc184720)

[3.2 LoopBackType 16](#_Toc184721)

[3.3 SeverityType 17](#_Toc184722)

[4 Super Classes 17](#_Toc184723)

[4.1 MwCurrentProblem 17](#_Toc184724)

[5 Notifications 19](#_Toc184725)

[5.1 AttributeValueChangedNotification 19](#_Toc184726)

[5.2 ObjectCreationNotification 20](#_Toc184727)

[5.3 ObjectDeletionNotification 21](#_Toc184728)

[5.4 ProblemNotification 22](#_Toc184729)

# TdmContainer

## TdmContainerCurrentProblems

Qualified Name: MicrowaveModel::ObjectClasses::TdmContainer::TdmContainerCurrentProblems

Applied stereotypes:

* OpenModelClass
* objectCreationNotification: NO
* objectDeletionNotification: NO
* support: MANDATORY

Table 1: Attributes for TdmContainerCurrentProblems

| **Attribute Name** | **Type DefaultValue** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| --- | --- | --- | --- | --- | --- |
| currentProblemList | ContainerCurrentProblemType  ./. | 0..\* | R | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: false * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY |  |

## MW\_TdmContainer\_Pac

Qualified Name: MicrowaveModel::ObjectClasses::TdmContainer::MW\_TdmContainer\_Pac

The TdmContainer\_Pac and its attached classes MUST be provided on management interfaces of microwave devices, which are transporting TDM traffic.

Applied stereotypes:

* OpenModelClass
* objectCreationNotification: YES
* objectDeletionNotification: YES
* support: CONDITIONAL\_MANDATORY
* condition: hybrid-microwave In case the microwave device allows Ethernet and native TDM transport in parallel, it has to support this feature on its management interface.

Table 2: Attributes for MW\_TdmContainer\_Pac

| **Attribute Name** | **Type DefaultValue** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| --- | --- | --- | --- | --- | --- |
| \_layerProtocol | LayerProtocol  ./. | 1 | RW | OpenModelAttribute   * partOfObjectKey: 1 * AVC: NO * isInvariant: false * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | CoreModel-CoreNetworkModule-ObjectClasses:NetworkElement/\_ltpRefList/\_lpList/uuid |
| \_tdmContainerCapability | TdmContainerCapability  ./. | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: false * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | See referenced class |
| \_tdmContainerConfiguration | TdmContainerConfiguration  ./. | 1 | RW | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: false * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | See referenced class |
| \_tdmContainerStatus | TdmContainerStatus  ./. | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: false * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | See referenced class |
| \_tdmContainerCurrentProblems | TdmContainerCurrentProblems  ./. | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: false * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | See referenced class |
| \_tdmContainerCurrentPerformance | TdmContainerCurrentPerformance  ./. | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: false * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | See referenced class |
| \_tdmContainerHistoricalPerformances | TdmContainerHistoricalPerformances  ./. | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: false * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | See referenced class |

## TdmContainerCapability

Qualified Name: MicrowaveModel::ObjectClasses::TdmContainer::TdmContainerCapability

Bundling is not available.

Applied stereotypes:

* OpenModelClass
* objectCreationNotification: NO
* objectDeletionNotification: NO
* support: MANDATORY

Table 3: Attributes for TdmContainerCapability

| **Attribute Name** | **Type DefaultValue** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| --- | --- | --- | --- | --- | --- |
| supportedTdmContainerTypesList | TdmContainerType  ./. | 1..\* | R | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | Lists the TDM containers that are supported. |
| supportedAlarmList | String  Supported alarms not yet defined. | 2..\* | R | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | Available alarms to be listed. Mandatory:'framingIsFaulty' and 'containerIsDown'. Further alarms might be added by the vendor. |
| supportedAlarms | String  Supported alarms not yet defined. | 1 | R | Deprecated  OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | Available alarms to be listed. Mandatory:'framingIsFaulty' and 'containerIsDown'. Further alarms might be added by the device. |

## TdmContainerConfiguration

Qualified Name: MicrowaveModel::ObjectClasses::TdmContainer::TdmContainerConfiguration

Applied stereotypes:

* OpenModelClass
* objectCreationNotification: NO
* objectDeletionNotification: NO
* support: MANDATORY

Table 4: Attributes for TdmContainerConfiguration

| **Attribute Name** | **Type DefaultValue** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| --- | --- | --- | --- | --- | --- |
| containerID | String  No TDM Flow associated yet. | 1 | RW | OpenModelAttribute   * partOfObjectKey: 0 * AVC: YES * isInvariant: false * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | ContainterID in Netconf must be the same as TDM Flow ID so a connection can be made between the two items, which separately exist in the controller. |
| containerType | TdmContainerType  ./. | 1 | RW | OpenModelAttribute   * partOfObjectKey: 0 * AVC: YES * isInvariant: false * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | Type of TDM container. |
| segmentID | SegmentIDType  ./. | 1 | RW | OpenModelAttribute   * partOfObjectKey: 0 * AVC: YES * isInvariant: false * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | Multiplicity = 1; One segment per TDM container; Type of segment must match type of container; |
| performanceMonitoringCollectionIsOn | Boolean  false | 1 | RW | OpenModelAttribute   * partOfObjectKey: 0 * AVC: YES * isInvariant: false * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | Enables measurement, collection, storage and access to performance data. |
| problemKindSeverityList | ContainerProblemSeverityType  ./. | 2..\* | RW | OpenModelAttribute   * partOfObjectKey: 0 * AVC: YES * isInvariant: false * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | Severity of the problem to be configured. |

## TdmContainerHistoricalPerformances

Qualified Name: MicrowaveModel::ObjectClasses::TdmContainer::TdmContainerHistoricalPerformances

Aggregated performance information of the TDM container for a pre-defined measurement interval.

Applied stereotypes:

* OpenModelClass
* objectCreationNotification: NO
* objectDeletionNotification: NO
* support: MANDATORY

Table 5: Attributes for TdmContainerHistoricalPerformances

| **Attribute Name** | **Type DefaultValue** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| --- | --- | --- | --- | --- | --- |
| historicalPerformanceDataList | ContainerHistoricalPerformanceType  ./. | 0..\* | R | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: false * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY |  |

## TdmContainerStatus

Qualified Name: MicrowaveModel::ObjectClasses::TdmContainer::TdmContainerStatus

Applied stereotypes:

* OpenModelClass
* objectCreationNotification: NO
* objectDeletionNotification: NO
* support: MANDATORY

Table 6: Attributes for TdmContainerStatus

| **Attribute Name** | **Type DefaultValue** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| --- | --- | --- | --- | --- | --- |
| lastStatusChange | DateTime  2010-11-20T14:00:00+01:00 | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: false * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | Time the Container entered its current operational status. \_format:yyyyMMddhhmmss.s[Z|{+|-}HHMm]; yyyy='0000'..'9999' year; MM='01'..'12' month; dd='01'..'31' day; hh='00'..'23' hour; mm='00'..'59' minute; ss='00'..'59' second; s='.0'..'.9'tenth of second (set to '.0' if EMS or NE cannot support this granularity); Z='Z' indicates UTC (rather than local time); {+|-}='+' or '-' delta from UTC; HH='00'..'23' time zone difference in hours; Mm='00'..'59' time zone difference in minutes. |

## TdmContainerCurrentPerformance

Qualified Name: MicrowaveModel::ObjectClasses::TdmContainer::TdmContainerCurrentPerformance

Aggregated performance information of the TDM container at a particular moment.

Applied stereotypes:

* OpenModelClass
* objectCreationNotification: NO
* objectDeletionNotification: NO
* support: MANDATORY

Table 7: Attributes for TdmContainerCurrentPerformance

| **Attribute Name** | **Type DefaultValue** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| --- | --- | --- | --- | --- | --- |
| currentPerformanceDataList | ContainerCurrentPerformanceType  ./. | 1..2 | R | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: false * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | At least values of the counters, which are reset every 15 minutes, are to be provided. If available, the current values of the counters, which are reset every 24 hour, can be provided, too. |

# Data Types

## ContainerCurrentPerformanceType

Qualified Name: MicrowaveModel::TypeDefinitions::ContainerCurrentPerformanceType

Turns performance information into current performance information by inheriting from OTN\_CurrentData.

Table 8: Attributes for ContainerCurrentPerformanceType

| **Attribute Name** | **Type DefaultValue** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| --- | --- | --- | --- | --- | --- |
| performanceData | ContainerPerformanceType  ./. | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY |  |

## ContainerCurrentProblemType

Qualified Name: MicrowaveModel::TypeDefinitions::ContainerCurrentProblemType

Table 9: Attributes for ContainerCurrentProblemType

| **Attribute Name** | **Type DefaultValue** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| --- | --- | --- | --- | --- | --- |
| problemName | String  Problem name not specified. | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | Name of the alarm according to Container::ContainerCapability::supportedAlarms |

## ContainerHistoricalPerformanceType

Qualified Name: MicrowaveModel::TypeDefinitions::ContainerHistoricalPerformanceType

Turns performance information into historical performance information by inheriting from OTN\_HistoryData.

Table 10: Attributes for ContainerHistoricalPerformanceType

| **Attribute Name** | **Type DefaultValue** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| --- | --- | --- | --- | --- | --- |
| performanceData | ContainerPerformanceType  ./. | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY |  |

## ContainerPerformanceType

Qualified Name: MicrowaveModel::TypeDefinitions::ContainerPerformanceType

Consolidated performance information of the Container.

Table 11: Attributes for ContainerPerformanceType

| **Attribute Name** | **Type DefaultValue** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| --- | --- | --- | --- | --- | --- |
| txEthernetBytesMaxS | Integer  -1 | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: LENGTH\_32\_BIT * unit: Bytes/s * support: MANDATORY | Counts the number of Bytes of Ethernet traffic (before header compression) transmitted within a second and keeps the highest value within the measurement period. Field to be left blank for all types of TDM containers. |
| txEthernetBytesMaxM | Integer  -1 | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: LENGTH\_64\_BIT * unit: Bytes/min * support: MANDATORY | Counts the number of Bytes of Ethernet traffic (before header compression) transmitted within a minute and keeps the highest value with in the measurement period. Field to be left blank for all types of TDM containers. |
| txEthernetBytesSum | Integer  -1 | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: LENGTH\_64\_BIT * unit: Bytes * support: MANDATORY | Total number of Bytes of Ethernet traffic (before header compression) transmitted (in direction out of the device) during the measurement period. Field to be left blank for all types of TDM containers. |
| timePeriod | Integer  -1 | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: LENGTH\_32\_BIT * unit: s * support: MANDATORY | Total length of the measurement period in seconds. |

## ContainerProblemSeverityType

Qualified Name: MicrowaveModel::TypeDefinitions::ContainerProblemSeverityType

Table 12: Attributes for ContainerProblemSeverityType

| **Attribute Name** | **Type DefaultValue** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| --- | --- | --- | --- | --- | --- |
| problemKindName | String  ./. | 1 | RW | OpenModelAttribute   * partOfObjectKey: 1 * AVC: NA * isInvariant: true * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | Name of the alarm according to Container::ContainerCapability::supportedAlarms |
| problemKindSeverity | SeverityType  WARNING | 1 | RW | OpenModelAttribute   * partOfObjectKey: 0 * AVC: YES * isInvariant: false * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | Severity of this type of alarm. |

## ContainerType

Qualified Name: MicrowaveModel::TypeDefinitions::ContainerType

* Obsolete

Table 13: Attributes for ContainerType

| **Attribute Name** | **Type DefaultValue** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| --- | --- | --- | --- | --- | --- |
| containerName | String  ./. | 1 | R | OpenModelAttribute   * partOfObjectKey: 1 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | Names to be chosen from the following list: 'ethernet','e1','t1','j1','e3','ds3','stm1','cpri1','cpri2','cpri3','cpri4','cpri5','cpri6' or 'cpri7' |
| numberOfTimeSlotsRequired | Integer  -1 | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: LENGTH\_16\_BIT * unit: timeslots * support: MANDATORY | Number of time slots required for transporting this type of container. Value must be calculated by the vendor after defining the timeSlotCapacity. For containers of fixed size: numberOfTimeSlotsRequired = required bandwidth of the container divided by timeSlotCapacity. For containers of variable size the minimum (most probably 1) is to be stated. |
| tdmTimeSlotsIsRequired | Boolean  false | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | Shall be set to '1', if this container type requires bandwidth (times slots) reserved for TDM transport. |
| bundlingIsAvail | Boolean  false | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | If it is possible to combine transport resources of several radio links to transport this container type, this attribute shall be set to '1'. |

## SegmentIDType

Qualified Name: MicrowaveModel::TypeDefinitions::SegmentIDType

Identifies the segments, which are used to transport the container.

Table 14: Attributes for SegmentIDType

| **Attribute Name** | **Type DefaultValue** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| --- | --- | --- | --- | --- | --- |
| structureIdRef | UniversalId  ./. | 1 | RW | OpenModelAttribute   * partOfObjectKey: 1 * AVC: YES * isInvariant: false * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY |  |
| segmentIdRef | Integer  ./. | 1 | RW | OpenModelAttribute   * partOfObjectKey: 2 * AVC: YES * isInvariant: false * valueRange: no range constraint * bitLength: LENGTH\_16\_BIT * unit: no unit defined * support: MANDATORY | Combinations of structureId and segmentId must be unique inside the device to assure that every resource is used just once. |

## SegmentStatusType

Qualified Name: MicrowaveModel::TypeDefinitions::SegmentStatusType

Table 15: Attributes for SegmentStatusType

| **Attribute Name** | **Type DefaultValue** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| --- | --- | --- | --- | --- | --- |
| segmentStatusTypeId | Integer  ./. | 1 | R | OpenModelAttribute   * partOfObjectKey: 1 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: LENGTH\_16\_BIT * unit: no unit defined * support: MANDATORY |  |
| segmentIsReservedForTdm | Boolean  false | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: false * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | The number of segments, which is configured by Structure::StructureConfiguration::tdmReservedNumberOfSegements, has to be reserved for TDM. Starting from the lowest index value, these segments have to be marked with a 'true' in segmentIsReservedForTdm. |
| operationalStatus | OperationalState  DISABLED | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: false * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | Current operational status of each segment. |
| obsoletePriorityClass | Integer  -1 | 1 | R | Obsolete  OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: false * valueRange: no range constraint * bitLength: LENGTH\_8\_BIT * unit: no unit defined * support: MANDATORY | PriorityClass as inherited from the associated Container::ContainerConfiguration::priorityClass. In case the device is capable of adapting the sequence, in which segments are being dropped in case of decreasing capacity of the air interface, priorityClass shall be considered, while calculating the dropOrderRank. |
| obsoleteDropOrderRank | Integer  -1 | 1 | R | Obsolete  OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: false * valueRange: no range constraint * bitLength: LENGTH\_16\_BIT * unit: no unit defined * support: MANDATORY | In case the device is NOT capable of adapting the sequence, in which segments are being dropped in case of decreasing capacity of the air interface, dropOrderRank is number of segments minus sequence number of the segment. In case the device is capable of adapting the sequence, dropOrderRank has to be calculated by the device in dependency to the assigned priorityClass. \_unique: within Structure::StructureStatus::segmentStatusList |

## TdmContainerType

Qualified Name: MicrowaveModel::TypeDefinitions::TdmContainerType

Table 16: Attributes for TdmContainerType

| **Attribute Name** | **Type DefaultValue** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| --- | --- | --- | --- | --- | --- |
| tdmContainerName | String  ./. | 1 | R | OpenModelAttribute   * partOfObjectKey: 1 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | Names to be chosen from the following list: 'e1','t1','j1','e3','t3','stm1','cpri1','cpri2','cpri3','cpri4','cpri5','cpri6' or 'cpri7' |
| tdmContainerSize | Integer  -1 | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: LENGTH\_32\_BIT * unit: kbit/s * support: MANDATORY | Capacity required for transporting this type of container (in kbit/s). Values to be chosen from the following list: '2048','1544','34000','44736 ','155520','614400','1228800','2457600','3072000','4915200','6144000' or '9830400; |

## TdmStructureType

Qualified Name: MicrowaveModel::TypeDefinitions::TdmStructureType

Table 17: Attributes for TdmStructureType

| **Attribute Name** | **Type DefaultValue** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| --- | --- | --- | --- | --- | --- |
| tdmStructureName | String  ./. | 1 | R | OpenModelAttribute   * partOfObjectKey: 1 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | Names to be chosen from the following list: 'e1','t1','j1','e3','ds3','stm1','cpri1','cpri2','cpri3','cpri4','cpri5','cpri6' or 'cpri7' |
| tdmSegmentSize | Integer  -1 | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: LENGTH\_32\_BIT * unit: kbit/s * support: MANDATORY | Size of the TDM segment in kbit/s. Values to be chosen from the following list: '2048','1544','34000','44736 ','155520','614400','1228800','2457600','3072000','4915200','6144000' or '9830400; |
| maxNumberOfSegmentsReservable | Integer  -1 | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: LENGTH\_8\_BIT * unit: segments * support: MANDATORY | Device specific maximum number of segments (not depending on current air interface configuration) that can be reserved for this type of segment on a single air interface. |

# Enumeration Types

## GranularityPeriodType

Qualified Name: MicrowaveModel::TypeDefinitions::GranularityPeriodType

The enumeration with the options for granularity period of the performance data.

Contains Enumeration Literals:

* UNKNOWN:
* PERIOD-15-MIN:
* PERIOD-24-HOURS:

## LoopBackType

Qualified Name: MicrowaveModel::TypeDefinitions::LoopBackType

Contains Enumeration Literals:

* RF\_TO\_REMOTE:
  + Returning the header information of the remote site back to the remote site on the radio interface between both outdoor units.
* RF\_TO\_LOCAL:
  + Returning the header information of the local site back to the local site on the radio interface between both outdoor units.
* IF\_TO\_REMOTE:
  + Returning the header information of the remote site back to the remote site on the intermediate frequency interface between local indoor unit and outdoor unit.
* IF\_TO\_LOCAL:
  + Returning the header information of the local site back to the local site on the intermediate frequency interface between local indoor unit and outdoor unit.
* NONE:
* IF:
  + Intermediate Frequency on the interface between indoor and outdoor unit.
    - Deprecated
* RF:
  + Radio Frequency on the interface between outdoor unit and outdoor unit at the remote site.
    - Deprecated
* NON:
  + - Deprecated

## SeverityType

Qualified Name: MicrowaveModel::TypeDefinitions::SeverityType

According to ITU-T M.3160

Contains Enumeration Literals:

* NON\_ALARMED:
* WARNING:
* MINOR:
* MAJOR:
* CRITICAL:

# Super Classes

## MwCurrentProblem

Qualified Name: MicrowaveModel::ObjectClasses::SuperClasses::MwCurrentProblem

Applied stereotypes:

* OpenModelClass
* objectCreationNotification: NO
* objectDeletionNotification: NO
* support: MANDATORY

Table 18: Attributes for MwCurrentProblem

| **Attribute Name** | **Type DefaultValue** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| --- | --- | --- | --- | --- | --- |
| sequenceNumber | Integer  ./. | 1 | R | OpenModelAttribute   * partOfObjectKey: 1 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: LENGTH\_32\_BIT * unit: no unit defined * support: MANDATORY | Unique sequence number of the current problem object. |
| timeStamp | DateTime  2010-11-20T14:00:00+01:00 | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | Time and date of the problem. \_format:yyyyMMddhhmmss.s[Z|{+|-}HHMm]; yyyy='0000'..'9999' year; MM='01'..'12' month; dd='01'..'31' day; hh='00'..'23' hour; mm='00'..'59' minute; ss='00'..'59' second; s='.0'..'.9'tenth of second (set to '.0' if EMS or NE cannot support this granularity); Z='Z' indicates UTC (rather than local time); {+|-}='+' or '-' delta from UTC; HH='00'..'23' time zone difference in hours; Mm='00'..'59' time zone difference in minutes. |
| problemSeverity | SeverityType  WARNING | 1 | R | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | Severity of the alarm. |

# Notifications

## AttributeValueChangedNotification

Qualified Name: MicrowaveModel::Notifications::AttributeValueChangedNotification

To be sent when an attribute has changed and one or more controllers have to update their data.

Applied stereotypes:

* OpenModelNotification
* triggerConditionList: invalid
* support: MANDATORY

Table 19: Attributes for AttributeValueChangedNotification

| **Attribute Name** | **Type DefaultValue** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| --- | --- | --- | --- | --- | --- |
| counter | Integer  -1 | 1 | RW | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: LENGTH\_32\_BIT * unit: no unit defined * support: MANDATORY | Counts attribute value changed notifications. |
| timeStamp | DateTime  2010-11-20T14:00:00+01:00 | 1 | RW | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY |  |
| objectIdRef | UniversalId  ./. | 1 | RW | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | ID of the affected MW\_AirInterface\_Pac, MW\_AirInterfaceDiversity\_Pac, MW\_Structure\_Pac, MW\_PureEthernetStructure\_Pac, MW\_HybridMwStructure\_Pac, MW\_Container\_Pac, MW\_EthernetContainer\_Pac or MW\_TdmContainer\_Pac. |
| attributeName | String  Attribute name not specified. | 1 | RW | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | Name of the attribute that has been changed. |
| newValue | String  New value not specified. | 0..1 | RW | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | Attribute value converted to a string (xml, json, ...) |

## ObjectCreationNotification

Qualified Name: MicrowaveModel::Notifications::ObjectCreationNotification

To be sent when a new MW\_AirInterface\_Pac, MW\_AirInterfaceDiversity\_Pac, MW\_Structure\_Pac, MW\_PureEthernetStructure\_Pac, MW\_HybridMwStructure\_Pac, MW\_Container\_Pac, MW\_EthernetContainer\_Pac or MW\_TdmContainer\_Pac has to be instancieted in the controller.

Applied stereotypes:

* OpenModelNotification
* triggerConditionList: invalid
* support: MANDATORY

Table 20: Attributes for ObjectCreationNotification

| **Attribute Name** | **Type DefaultValue** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| --- | --- | --- | --- | --- | --- |
| counter | Integer  -1 | 1 | RW | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: LENGTH\_32\_BIT * unit: no unit defined * support: MANDATORY | Counts object creation notifications. |
| timeStamp | DateTime  2010-11-20T14:00:00+01:00 | 1 | RW | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY |  |
| objectIdRef | UniversalId  ./. | 1 | RW | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | ID of the affected MW\_AirInterface\_Pac, MW\_AirInterfaceDiversity\_Pac, MW\_Structure\_Pac, MW\_PureEthernetStructure\_Pac, MW\_HybridMwStructure\_Pac, MW\_Container\_Pac, MW\_EthernetContainer\_Pac or MW\_TdmContainer\_Pac. |
| objectType | String  Type of created object not specified. | 1 | RW | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | Type of Object to be chosen from the following list of values: 'MW\_AirInterface\_Pac', 'MW\_AirInterfaceDiversity\_Pac', 'MW\_Structure\_Pac', 'MW\_PureEthernetStructure\_Pac', 'MW\_HybridMwStructure\_Pac', 'MW\_Container\_Pac', 'MW\_EthernetContainer\_Pac' or 'MW\_TdmContainer\_Pac'. |

## ObjectDeletionNotification

Qualified Name: MicrowaveModel::Notifications::ObjectDeletionNotification

To be sent when a new MW\_AirInterface\_Pac, MW\_AirInterfaceDiversity\_Pac, MW\_Structure\_Pac, MW\_PureEthernetStructure\_Pac, MW\_HybridMwStructure\_Pac, MW\_Container\_Pac, MW\_EthernetContainer\_Pac or MW\_TdmContainer\_Pac instance has to be deleted in the controller.

Applied stereotypes:

* OpenModelNotification
* triggerConditionList: invalid
* support: MANDATORY

Table 21: Attributes for ObjectDeletionNotification

| **Attribute Name** | **Type DefaultValue** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| --- | --- | --- | --- | --- | --- |
| counter | Integer  -1 | 1 | RW | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: LENGTH\_32\_BIT * unit: no unit defined * support: MANDATORY | Counts object deletion notifications. |
| timeStamp | DateTime  2010-11-20T14:00:00+01:00 | 1 | RW | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY |  |
| objectIdRef | UniversalId  ./. | 1 | RW | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | ID of the affected MW\_AirInterface\_Pac, MW\_AirInterfaceDiversity\_Pac, MW\_Structure\_Pac, MW\_PureEthernetStructure\_Pac, MW\_HybridMwStructure\_Pac, MW\_Container\_Pac, MW\_EthernetContainer\_Pac or MW\_TdmContainer\_Pac. |

## ProblemNotification

Qualified Name: MicrowaveModel::Notifications::ProblemNotification

To be sent when a problem occurs at a MW\_AirInterface\_Pac, MW\_AirInterfaceDiversity\_Pac, MW\_Structure\_Pac, MW\_PureEthernetStructure\_Pac, MW\_HybridMwStructure\_Pac, MW\_Container\_Pac, MW\_EthernetContainer\_Pac or MW\_TdmContainer\_Pac.

Applied stereotypes:

* OpenModelNotification
* triggerConditionList: invalid
* support: MANDATORY

Table 22: Attributes for ProblemNotification

| **Attribute Name** | **Type DefaultValue** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| --- | --- | --- | --- | --- | --- |
| counter | Integer  -1 | 1 | RW | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: LENGTH\_32\_BIT * unit: no unit defined * support: MANDATORY | Counts problem notifications |
| timeStamp | DateTime  2010-11-20T14:00:00+01:00 | 1 | RW | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY |  |
| objectIdRef | UniversalId  ./. | 1 | RW | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | ID of the affected MW\_AirInterface\_Pac, MW\_AirInterfaceDiversity\_Pac, MW\_Structure\_Pac, MW\_PureEthernetStructure\_Pac, MW\_HybridMwStructure\_Pac, MW\_Container\_Pac, MW\_EthernetContainer\_Pac or MW\_TdmContainer\_Pac. |
| problem | String  Problem name not specified. | 1 | RW | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | Name of the problem according to AirInterface::AirInterfaceCapability::supportedAlarms or AirInterfaceDiversity::AirInterfaceDiversityCapability::supportedAlarms or Structure::StructureCapability::supportedAlarms or PureEthernetStructure::PureEthernetStructureCapability::supportedAlarms or HybridMwStructure::HybridMwStructureCapability::supportedAlarms or Container::ContainerCapability::supportedAlarms or EthernetContainer::EthernetContainerCapability::supportedAlarms or TdmContainer::TdmContainerCapability::supportedAlarms. |
| severity | SeverityType  WARNING | 1 | RW | OpenModelAttribute   * partOfObjectKey: 0 * AVC: NO * isInvariant: true * valueRange: no range constraint * bitLength: NA * unit: no unit defined * support: MANDATORY | Severity of the problem according to AirInterface::AirInterfaceConfiguration::problemSeverityList, AirInterfaceDiversity::AirInterfaceDiversityConfiguration::problemSeverityList, Structure::StructureConfiguration::problemSeverityList, PureEthernetStructure::PureEthernetStructureConfiguration::problemSeverityList, HybridMwStructure::HybridMwStructureConfiguration::problemSeverityList, Container::ContainerConfiguration::problemSeverityList, EthernetContainer::EthernetContainerConfiguration::problemSeverityList or TdmContainer::TdmContainerConfiguration::problemSeverityList |