Content

[2 Classes 1](#_Toc154171243)

[2.1 TdmContainerCapability 1](#_Toc154171244)

[2.2 TdmContainerConfiguration 2](#_Toc154171245)

[2.3 TdmContainerKind 4](#_Toc154171246)

[2.4 TdmContainerLpSpec 4](#_Toc154171247)

[2.5 TdmContainerStatus 5](#_Toc154171248)

[2.6 TdmContainer\_Pac 6](#_Toc154171249)

[3 Data Types 7](#_Toc154171250)

[4 Enumeration Types 7](#_Toc154171251)

[4.1 InterfaceStatusType 7](#_Toc154171252)

[4.2 LayerProtocolNameType 8](#_Toc154171253)

[4.3 LoopBackType 8](#_Toc154171254)

[5 Primitive Types 8](#_Toc154171255)

# Classes

## TdmContainerCapability

Applied stereotypes:

* OpenModelClass
* support: MANDATORY
* OpenInterfaceModelClass
* objectCreationNotification: NO
* objectDeletionNotification: NO

Attributes for TdmContainerCapability

Table 1: Attributes for TdmContainerCapability

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| \_supportedTdmContainerKindList | TdmContainerKind  ./. | 1..\* | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA | Lists the TDM containers that are supported. |
| adminShutDownIsAvail | Boolean  false | 1 | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA | true = Manual switching on and off of the interface without deleting it (underlying OSI network layers are also not affected) is available. |
| supportedLoopBackKindList | LoopBackType  ./. | 1..3 | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA | List of supported kinds of looping back. |
| maintenanceTimerRange | String  Range of the maintenance timer not yet defined. | 1 | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA | Available time periods for maintenance configurations to be described. Concrete values shall be separated by commas (e.g. '10, 60, 360'). Ranges shall be expressed as two values separated by a minus (e.g. '10-360'). |

## TdmContainerConfiguration

Applied stereotypes:

* OpenModelClass
* support: MANDATORY
* OpenInterfaceModelClass
* objectCreationNotification: NO
* objectDeletionNotification: NO

Attributes for TdmContainerConfiguration

Table 1: Attributes for TdmContainerConfiguration

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| interfaceName | String  Interface name not yet defined. | 1 | RW | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA | Description of the interface, could be a name, could be a number. Free text field to be filled by the operator. |
| interfaceIsOn | Boolean  false | 1 | RW | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA | Only relevant if (adminShutDownIsAvail==1). 1 = Activation of the interface. 0 = De-activation of the interface without deleting it (underlying OSI network layers are not affected). |
| \_tdmContainerKind | TdmContainerKind  ./. | 1 | RW | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  PassedByReference  OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA | Type of TDM container. |
| segmentNumber | Integer  -1 | 1 | RW | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: YES  • bitLength: LENGTH\_16\_BIT | Serving TDM structure is identified by LogicalTerminationPoint::\_serverLtpRefList (Multiplicity = 1; One segment per TDM container). Serving Segment is identified by segmentID attribute. Type of segment must match type of container. |
| loopBackKindOn | LoopBackType  NOT\_YET\_DEFINED | 1 | RW | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA | Maintenance Feature. Configuration of a loop back of TDM time slots on this interface. |
| maintenanceTimer | Integer  -1 | 1 | RW | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: s  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: YES  • bitLength: LENGTH\_32\_BIT | Time of existence of any maintenance configuration. 0 = maintenance timer is switched off. Valid values are defined in \*Capability::maintenanceTimerRange. |

## TdmContainerKind

Applied stereotypes:

* OpenModelClass
* support: MANDATORY
* OpenInterfaceModelClass
* objectCreationNotification: NO
* objectDeletionNotification: NO

Attributes for TdmContainerKind

Table 1: Attributes for TdmContainerKind

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| tdmContainerName | String  ./. | 1 | R | OpenModelAttribute  • partOfObjectKey: 1  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA | Names to be chosen from the following list: 'e1','t1','j1','e3','t3','stm1','cpri1','cpri2','cpri3','cpri4','cpri5','cpri6' or 'cpri7' |
| tdmContainerSize | Integer  -1 | 1 | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: kbit/s  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: LENGTH\_32\_BIT | Capacity required for transporting this type of container (in kbit/s). Values to be chosen from the following list: '2048','1544','34000','44736 ','155520','614400','1228800','2457600','3072000','4915200','6144000' or '9830400; |

## TdmContainerLpSpec

The TdmContainerLpSpec and its attached classes MUST be provided on management interfaces of microwave devices, which are transporting TDM traffic.

Applied stereotypes:

* OpenModelClass
* support: MANDATORY
* OpenInterfaceModelClass
* objectCreationNotification: YES
* objectDeletionNotification: YES

Attributes for TdmContainerLpSpec

Table 1: Attributes for TdmContainerLpSpec

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| \_tdmContainer\_Pac | TdmContainer\_Pac  ./. | 1 | RW | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA | See referenced class |

## TdmContainerStatus

Applied stereotypes:

* OpenModelClass
* support: MANDATORY
* OpenInterfaceModelClass
* objectCreationNotification: NO
* objectDeletionNotification: NO

Attributes for TdmContainerStatus

Table 1: Attributes for TdmContainerStatus

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| interfaceStatus | InterfaceStatusType  NOT\_YET\_DEFINED | 1 | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA | Operational status of the interface. |
| loopBackKindUp | LoopBackType  NOT\_YET\_DEFINED | 1 | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: false  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: YES  • bitLength: NA | The currently active (not just configured) type of loop back. |

## TdmContainer\_Pac

Applied stereotypes:

* OpenModelClass
* support: MANDATORY
* OpenInterfaceModelClass
* objectCreationNotification: NO
* objectDeletionNotification: NO

Attributes for TdmContainer\_Pac

Table 1: Attributes for TdmContainer\_Pac

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Attribute Name** | **Type** | **Multiplicity** | **Access** | **Stereotypes** | **Description** |
| \_tdmContainerCapability | TdmContainerCapability  ./. | 1 | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA | See referenced class |
| \_tdmContainerConfiguration | TdmContainerConfiguration  ./. | 1 | RW | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA | See referenced class |
| \_tdmContainerStatus | TdmContainerStatus  ./. | 1 | R | OpenModelAttribute  • partOfObjectKey: 0  • isInvariant: true  • valueRange: no range constraint  • unit: no unit defined  • support: MANDATORY  OpenInterfaceModelAttribute  • AVC: NO  • bitLength: NA | See referenced class |

# Enumeration Types

## InterfaceStatusType

Current Interface Status

Contains Enumeration Literals:

* UP:
  + Ready to pass packets. It is expected that the LogicalTerminationPoint::operationalState attribute is expressing this logical layer being available for use (means: ENABLED), while this value occurs.
* DOWN:
  + The interface does not pass any packets. It is expected that the LogicalTerminationPoint::operationalState attribute is expressing this logical layer being NOT available for use (means: DISABLED), while this value occurs.
* TESTING:
  + In some test mode. No operational packets can be passed. It is expected that the LogicalTerminationPoint::operationalState attribute is expressing this logical layer being NOT available for use (means: DISABLED), while this value occurs.
* UNKNOWN:
  + Status cannot be determined for some reason. While this value occurs, the LogicalTerminationPoint::operationalState attribute, which is expressing the availability of the logical layer for being used, might have either ENABLED or DISABLED as value.
* DORMANT:
  + Waiting for some external event. It is expected that the LogicalTerminationPoint::operationalState attribute is expressing this logical layer being available for use (means: ENABLED), while this value occurs.
* NOT\_PRESENT:
  + Some component (typically hardware) is missing. It is expected that the LogicalTerminationPoint::operationalState attribute is expressing this logical layer being NOT available for use (means: DISABLED), while this value occurs.
* NOT\_YET\_DEFINED:
  + While this value occurs, the LogicalTerminationPoint::operationalState attribute, which is expressing the availability of the logical layer for being used, might have either ENABLED or DISABLED as value.

## LayerProtocolNameType

A controlled list of LayerProtocol names.

Contains Enumeration Literals:

* LAYER\_PROTOCOL\_NAME\_TYPE\_TDM\_CONTAINER\_LAYER:

## LoopBackType

Contains Enumeration Literals:

* NONE:
* BACK\_TO\_LOCAL:
  + Returning the TDM time slots of the local site on the outgoing interface back to the local site.
* BACK\_TO\_REMOTE:
  + Returning the incoming TDM time slots back to the remote site.
* NOT\_YET\_DEFINED: